|  |  |
| --- | --- |
| **Date of asbestos register:** | Click or tap to enter a date. |
| **NOTE: A demolition or refurbishment survey should be carried out by a competent person before undertaking refurbishment or demolition work.** |
| **Workplace address:** | Click or tap here to enter text. | **Competent person** | **Workplace owner/manager** |
| **Name:** | Click or tap here to enter text. | **Name:** | Click or tap here to enter text. |
| **Contact details:** | Click or tap here to enter text. | **Position:** | Click or tap here to enter text. |
| **Licence No:** | Click or tap here to enter text. | **Contact details:** | Click or tap here to enter text. |
| **Areas not assessed:** | Describe the location of areas not assessed during the asbestos survey and provide an explanation as to why. |
| **Asbestos related documents:** | Link or details about how to access other documents e.g. asbestos survey report, Asbestos Management Plan, asbestos clearance certificates, asbestos removal control plan, and Safe Work Method Statement. |
| **Consultation:** | Outline of consultation with workers and any representatives. Attach minutes of relevant meetings. |
| **Date** | **Sample No.** | **Type of material identified or assumed and amount** | **Friable or** **non-friable asbestos** | **Condition of asbestos** | **Specific location of identified or assumed asbestos** | **Photo No.** | **Notes** |
| Date of the survey. | Include the laboratory reference number if a sample was sent for testing.  | * Product type (e.g. cement sheet, vinyl tiles).
* Mineral type (e.g. chrysotile, tremolite, white, brown).
* Amount of material present(e.g. surface area, length, number of gaskets).
 | Choose an item. | * Condition (e.g. stable, poor, unknown).
* State of deterioration(e.g. minor, severe, weathering, cracks, peeling paint, material lifting to reveal asbestos).
* Surface coating(e.g. paint, vinyl).
* Describe if any treatment was used to prevent breakdown.
 | * Describe the location (inside or outside).
* If inside include room name or number and where in the room? (e.g. floor, east wall, boiler, etc).
* If outside (e.g. exterior wall, south facing, etc).
* Reference diagrams or building plans highlighting the location.
* State if material is labelled and colour coded to distinguish between friable and non-friable.
 | Include photos of the asbestos and ACM and cross reference by number.  | * State if the area is accessible.
* If area is not accessible, explain why it may contain asbestos.
* Probability of disturbing or damaging the asbestos (e.g. low, medium or high probability) from activities that would normally be carried out at the workplace.
* Management recommendations (e.g. restrict access, encapsulate, remove, maintain in good condition).
* Other details or instructions.
 |
| **Example:** |
| 21/11/2022 | S001 | Toilet cubicle door and partition. Approx. 4m2 | Non-friable | Stable condition, no deterioration, painted surface. | Ground floor bathroom. |  | Area accessible. Encapsulate to maintain in stable condition. **Remove prior to any refurbishment or demolition works.** |